





[](https://www.cirmall.com/articles/35838/)














Serial Monitor (Ctrl+Shift+M) 2->Send 115200 baud

It processes the values from the accelerometer and gyroscope to give us accurate 3D values ; i.e Yaw , Pitch and Roll.

